{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":84,"n_cols":6,"rows_kept":84,"merged":[[0,0,0,5],[1,0,1,5],[2,0,4,0],[2,1,4,1],[2,2,4,2],[2,3,4,3],[2,4,4,4],[2,5,4,5],[5,0,16,0],[5,1,8,1],[9,1,16,1],[17,0,22,0],[17,1,22,1],[23,0,83,0],[23,1,76,1],[77,1,83,1]],"flags":["formulas_cached_only"]}
["2025年上半年实验室机房建设汇总表"]
["工程仿真实验室（G508）+数字交通联合实验室（Q楼）+机器人模拟仿真实验室（D106）+虚拟现实与三维重建实验室（H403/405）+数字动画实训室（H409）"]
["院部","实验室名称","仪器设备名称","详细技术参数","单位","数量"]
[]
[]
["智慧交通现代产业学院","工程仿真实验室（G508）    技术咨询：吴芳芳 13866782885        邵老师  18255027137      ","电脑","1、CPU：≥16核心24线程，≥2.1GHz主频，三级缓存≥30MB；\n2、主板：全固态电容，B7系列芯片组或以上（非H系列)；\n3、接口：≥8个USB 接口（其中至少包含4个USB Type-A 3.2)\n，2个PS2，1个串口;\n4、硬盘：≥512GB固态硬盘，应冗余1个M.2固态盘位，2个3.5寸机械硬盘位；\n5、内存：≥16GB DDR4 3200MHZ,4内存插槽,最大支持128GB或以上；\n6、音频接口：提供前2后3共5个音频接口；\n7、显卡：≥RX550 4G;\n8、电源：峰值功率不低于500W；具备防雷及动态调整电压及有效节能的电压控制模块，电压89V-265V 之间可稳定正常工作,提供检验证明；\n9、机箱：立式机箱体积应在17L-30L之间，产品工作在空闲状态下，产品的声功率级应不超过 1.75 Bel，提供检验证明；\n10、原厂机房综合运维管理系统: 出厂自带网络同传，独立界面操作同传、还原等重要功能（非基于 Windows系统操作，响应文件中提供软件功能截图扫描件或影印件），支持双硬盘保护，支持机械硬盘、SSD硬盘、M.2硬盘、eMMC硬盘，支援双硬盘在进行PXE批量部署或者智能对拷时，接收端硬盘顺序和发送端硬盘顺序不一致时，提供手动修改硬盘顺序的功能，确保双硬盘对拷数据按照发送端存储方式对拷，保证所有计算机对拷完成后环境完全相同。支持系统自动还原，批量修改计算机名、IP，支持不同系统分配不同的IP，支持增量拷贝、断电续传、远程唤醒、远程重启、远程锁定、远程关机。支持任意机器作为主机对整个机房的维护，同传时可在同传界面直观的显示当前网络状况，方便网络传输故障点定位；为方便教学管理可支持屏幕锁定、键鼠锁定、光驱锁定及USB锁定，支持文件批量发送，支持发送消息及通知。集成软硬件资产管理功能，可查看机器的软硬件资产，并支持一键导出资产报表。具备考试模式。\n11、原厂数据管理系统：应具备硬盘设立独立加密分区功能、外置U盘分区加密功能、数据安全删除功能，基于硬件底层的数据安全擦除功能且保证硬盘数据擦除后不可恢复、一键系统恢复功能（非系统自带）。（提供功能截图）\n12、键鼠：USB光电抗菌鼠标；USB防水抗菌键盘；\n13、整机制造商三年上门维修服务，具备7*24小时400技术支持热线；\n14、显示器：≥21.5英寸IPS显示器三边窄边设计，与主机同品牌，黑色；取得护眼滤蓝光认证。\n15、保证设备稳定运行平均无故障运行时间不低于110万小时，提供检验证明；\n16、商用产品，黑色，原装非改配；以上技术参数提供官网链接、彩页、技术说明书等材料佐证。","台",61]
[null,null,"交换机","全千兆网络交换机","台",3]
[null,null,"设备安装调试（含原强弱电线路更换、综合布线）","实验室强弱电拆除及更换新的布线","项",1]
[null,null,"设备维护（配套设施、桌椅及环境改造）","实验室配套桌椅等","项",1]
[null,"数字交通联合实验室（Q楼）  技术咨询：黄先伟 13866106601  ","主机","处理器：Intel i7\n硬盘容量：1TB SSD+4T机械硬盘\n显卡型号：RTX 4060TI\n内存容量：128GB","台",21]
[null,null,"显示屏","27英寸/4K","台",21]
[null,null,"路由器",null,"台",2]
[null,null,"交换机","华三Mini s24-u(24口）","台",2]
[null,null,"插线排","公牛8位总控5米","个",5]
[null,null,"插线排","公牛8位总控1.8米","个",10]
[null,null,"网线/插排合理走线","网线+外包服务","项",1]
[null,null,"文化墙建设","定制","套",1]
["现代康养产业学院","机器人模拟仿真实验室（D106） 技术咨询：金文婷 13856512663   ","电脑","联想品牌机内存不低于16GB，固态硬盘容量不少于512GB","台",60]
[null,null,"嵌入式虚拟仿真平台","总体要求：仿真系统需包含“嵌入式原理仿真”和“嵌入式程序仿真”两大部分。原理仿真完成嵌入式处理器内部各个单元的工作原理展示与应用系统的仿真；程序仿真完成程序源码在目标应用系统上的仿真、调试功能。\n控制器原理仿真（投标时提供证明材料）\n要求每个控制器都能提供控制器内部的原理框图，改变对应寄存器的值可以实时反应在框图结构中。每个控制器涉及的寄存器都能查看寄存器位域结构，并且每个位域均可独立控制，并根据位域设置值影响仿真动画。仿真动画速度可调，支持慢速、中速、快速动画仿真，满足对动画速度的调节。\nGPIO控制器：支持信号发生器、示波器等测试工具，可对输入输出接口进行测试仿真。\nClock控制器：可以通过寄存器配置将各个时钟域输出时钟通过MCO引脚输出，并且可以用示波器测量时钟信号。\nUART控制器：带有数据缓存队列，可批量输入要发送的数据，控制器会依次将数据缓存队列中的数据发送出去。\n中断控制器：可以支持EXTI外部中断与事件及NVIC中断与异常管理，可支持模拟软件中断、GPIO管脚中断、系统异常等。\nDMA控制器、ADC控制器、I2C控制器、SPI控制器、基本定时器与通用控制器、FSMC控制器等支持配置和仿真的寄存器、FSMC可支持的仿真功能\n基础应用仿真（投标时提供软件截图证明材料）\n原理图仿真可支持通用模块、输入\\输出模块、接口模块、模拟电压模块、存储模块、传感器模块、外部扩展板等至少6种类型的外部设备。\nPCB图仿真支持查看顶层信号层、中间层信号层、底层信号层、顶层丝印层、底层丝印层、顶层助焊层、顶层阻焊层、底层阻焊层、边框层、钻孔层等各层图纸。\n电路板3D模型至少包含：继电器控制板、可调电源方波信号发生器、RS232串口、RS485串口、EEPROM、TMP125温度模块、风扇模块、空气温湿度、光强传感器、可调速风扇、LCD触摸屏等，模型数量≥13个。\n每个3D模型都是根据实际器件进行3D模型还原，还可将器件与主板进行分离，可更加直观的认识每个电子器件。\n3D应用场景仿真需支持3D器件接线，并可以使用示波器对主要信号进行测量。\n仿真软件可支持2D场景和3D场景下程序流程图仿真，每个流程中可配置当前流程要执行的程序操作。\n处理器原理仿真\n支持Cortex-M4处理器内核寄存器仿真，包含通用寄存器、栈指针寄存器、链接寄存器、程序计数器、程序状态寄存器、异常屏蔽寄存器、控制寄存器。\n支持处理器工作模式仿真，可支持特权模式、线程模式、主栈模式、线程栈模式，各模式间的切换规则。\n支持Cortex-M4处理器汇编指令集仿真，包含数据处理、分支跳转、内存访问、异常产生、特殊寄存器访问等指令仿真。\n综合项目案例仿真\n综合项目案例采用核心板+主板+外部扩展模块方式设计，可灵活扩展多种外部传感器。\n主板板载外设包含：不少于4个LED、不少于4个用户自定义按键、1个蜂鸣器、1个电位器、1个ESP8266 WiFi模组、1组外部IO扩展口、1组LCD屏幕接口。\n板载外部IO扩展口包含：1路UART接口、1路I2C接口、1路SPI接口、不少于3路ADC接口、不少于3路PWM接口。\n外部扩展板至少包含以下3D模型：空气温湿度扩展板、火焰传感器扩展板、光强传感器扩展板、可调速风扇扩展板、LED灯扩展板。\nPCB图仿真可支持核心板PCB图仿真、主板PCB图仿真、外部扩展板PCB图仿真；每个设备均可查看顶层信号层、中间层信号层、底层信号层、顶层丝印层、底层丝印层、顶层助焊层、顶层阻焊层、底层阻焊层、边框层、钻孔层等各层图纸。\n2D模式基础实验硬件接线\n硬件接线工程的创建、保存、导入，导出功能。\n每个器件的接线端子有接口名称提示功能。\n支持画线、拖拽、删除、清空等编辑功能。\n支持接线验证功能，错误位置提示功能，投标时提供截图证明。\n提供针对每个应用系统的程序仿真功能。程序仿真功能支持3种模式，分别是：仿真系统自动生成的工程源码仿真、自己根据IDE环境新创建的工程源码仿真、可执行文件（elf、bin）的仿真。在IDE环境中，可以实现程序源码的单步、断点、全速、暂停等功能，可以查看寄存器、内存的数值，可以查看反汇编功能。程序运行可以直接和应用系统关联，实现和应用系统之间的动态交互。\n可提供控制器原理、基础应用等实验资源：\n控制器原理包含：GPIO控制器实验、CLK控制器实验、UART控制器实验、EXTI控制器实验、NVIC控制器实验、DMA控制器实验等，实验数量≥20个；\n基础应用包含：按键输入实验、调压信号发生器实验、USB串口通信实验、土壤温湿度采集实验、按键中断实验、串口中断实验、DMA内存到内存实验、EEPROM实验（I2C中断方式）、模拟电压采集实验（ADC中断方式）、温度采集实验（SPI中断方式）、PWM风扇控制实验、输入脉宽捕获实验、输入脉冲计数实验等，实验数量≥27个；\n处理器原理包含：通用寄存器实验、栈指针寄存器实验、链接寄存器实验、程序计数器实验、程序状态寄存器实验、异常屏蔽寄存器实验、处理器工作模式实验等，实验数量≥12个；\n综合项目案例包含：智能灯光控制系统、智能大棚温控系统、火灾报警系统、自定义项目\n提供产品的原厂授权书，和原厂售后服务承诺函","点",30]
[null,null,"服务器","（1）机型：2U机架式服务器，推荐国产自研品牌；\n（2）处理器：配置2颗Intel Xeon 4314或以上处理器，单颗物理核心数≥16核，基本频率≥2.4GHz；\n（3）内存：配置≥256GB DDR4内存；支持≥32个DDR4内存插槽；\n（4）硬盘：配置≥2块512GB SATA SSD硬盘（系统盘），配置≥4块8T SATA HDD硬盘（数据盘）；支持≥20块3.5寸硬盘或≥45块2.5寸硬盘，可选支持≥2个SATA M.2或≥2个E1.S盘（短RSSD）\n（5）RAID：配置≥1张与服务器同品牌RAID阵列卡，≥2G缓存；\n（6）网口：配置≥4个千兆电口；支持≥1个OCP3.0网络模块，提供1Gb/10Gb/25Gb/40Gb/100Gb/200Gb多种网络接口选择， \n（7）性能：产品在SPEC max-jOPS测试中，最大性能指标不低于286000 \n（8）操作系统： win server 2016 标准版\n（9）数据库：sql server  2016 标准版","台",1]
[null,null,"电脑桌","定制","张",30]
[null,null,"凳子",null,"张",60]
[null,null,"线路改造和环境改造","必须联系实验室负责人看完现场后报价","间",1]
["数字创意现代产业学院","虚拟现实与三维重建实验室（H403/405）          技术咨询：张健 17705600792   ","Windows高性能工作站","CPU: Intel Core i9-13900K; GPU: NVIDIA RTX 4090 24GB; 主板: ASUS ROG Maximus Z790 Hero; 内存: 64GB DDR5; 存储: 1TB NVMe SSD + 4TB SATA HDD; 电源: 1000W; 散热: Noctua NH-D15","台",4]
[null,null,"Pico 4 Ultra","显示分辨率：4K+; 存储：256GB; 便携式设计","台",10]
[null,null,"HTC VIVE Focus Vision","分辨率：4K; 光学追踪","台",2]
[null,null,"HoloLens 2 开发者版","混合现实，支持全息影像; 开发工具兼容性","台",1]
[null,null,"Apple Vision Pro"," 支持全息显示和互动; Apple生态兼容","台",1]
[null,null,"Pico 4 Ultra 便携包","Pico 官方便携包,硬壳保护，便携性高","个",5]
[null,null,"VR串流充电线","USB 3.2 Gen 1 串流线 5米,高速充电与数据传输","根",25]
[null,null,"Pico 4近视眼镜配件","100-600度镜片,适配Pico 4设备，矫正视力","副",12]
[null,null,"Vision Pro 配件","600、400、200度镜片+保护仓,包含近视镜片，保护套，保修服务","套",1]
[null,null,"手柄电池","5号电池,VR手柄适配，支持长时间供电","件",80]
[null,null,"VR眼镜桌面收纳展示支架","桌面展示架,便于展示和保护VR眼镜","个",5]
[null,null,"VR眼镜一次性护脸布","100片/盒,卫生防护耗材","盒",20]
[null,null,"影石 Insta360 X4","支持4K分辨率，360°全景拍摄","台",2]
[null,null,"无人机","DJI Air 3S 畅飞套装,支持高清航拍与长续航","台",1]
[null,null,"佳能 R6 Mark 2 相机","高分辨率拍摄，支持动态捕捉","台",1]
[null,null,"相机镜头","RF24-70mm F2.8 L IS USM,高质量镜头，适配佳能R6相机","个",1]
[null,null,"三脚架","富图宝便携碳纤维三脚架,轻便耐用，适合户外使用","个",1]
[null,null,"高速存储SD卡","闪迪 128GB SD内存卡,支持高速数据写入","张",2]
[null,null,"高速存储TF卡","闪迪 256GB TF内存卡,适用于无人机或相机","张",1]
[null,null,"小型摄影棚","80cm×60cm,适合静物摄影，提供均匀光线","个",1]
[null,null,"多色3D打印机","拓竹X1系列,支持多种材料与颜色打印","台",2]
[null,null,"3D打印机耗材","适配拓竹X1,PLA；PA12 CF；PA12 CF Support；","套",5]
[null,null,"戴尔显示器","27英寸，4K分辨率","台",5]
[null,null,"Sony 显示器","77英寸，OLED面板","台",1]
[null,null,"电视可移动支架","65-86寸适配,便于大屏幕移动展示","个",1]
[null,null,"打印机","HP LaserJet Pro MFP M428fdw,多功能激光打印机，支持无线连接","台",1]
[null,null,"Windows工作站工作台","办公桌：可升降桌子，尺寸160×80cm；椅子：可调节","套",4]
[null,null,"三维重建扫描工作台","适配三维扫描设备，尺寸定制，200*80cm，可升降","套",1]
[null,null,"会议工作台","木质会议桌尺寸：2米×1米，","套",1]
[null,null,"圆形矮凳","可旋转、带滚轮，无靠背，便于灵活移动","套",10]
[null,null,"无线键鼠套装","高精度，支持多设备连接","套",5]
[null,null,"可移动白板","适合教学与演示  白板+支架180*90cm","个",1]
[null,null,"白板笔","多色选择，适合白板书写","支",20]
[null,null,"独立开关插座","6位插座，安全多用插座","个",10]
[null,null,"路由器","支持WiFi 6，高速无线网络支持，最高支持2000M以上","台",2]
[null,null,"交换机","48口千兆以太网交换机，支持局域网高速传输","台",2]
[null,null,"网线","超六类网线，支持高速网络连接","米",200]
[null,null,"展柜","适合设备展示与存储","个",1]
[null,null,"设备存储柜","锁闭式设计，适合存放精密设备","个",2]
[null,null,"128GB 优盘","USB3.2 Gen；读速220MB/s 写速100MB/s","张",20]
[null,null,"2T 固态移动硬盘","Type-c接口；NVMe读速1050MB/s","张",4]
[null,null,"绿联4K 无线投屏器","50米远距离稳定传输，支持4K30Hz，即插即用，带独立3.5mm接口；绿联CM586","个",1]
[null,null,"VR设备存储柜","HTC VIVE VR眼镜充电柜 Pico头盔消毒柜 VR头显存储柜 USB快捷充电 紫外线消毒 滚轮便携移动 VR存储箱 VR 30个位置（充电+消毒）","个",1]
[null,null,"RF 85mm 相机镜头","RF 85mm F1.2 L USM","个",1]
[null,null,"高性能服务器","满足搭载了5块NVIDIA RTX 4090 24GB；能够支持4个独立服务；用于数字人模型训练","套",1]
[null,null,"整套数字人2D、3D采集工具","满足对虚拟数字人的采集；","套",1]
[null,null,"学生计算机","CPU: I Intel Core i7-13700F; GPU: NVIDIA RTX 4070 Super; 主板: ASUS TUF GAMING B660M; 内存: 32GB DDR4; 存储: 512GB NVMe SSD + 1TB HDD; 电源: 750W 或800 Gold; 散热: Thermalright(利民)；显示器：2k 24寸；鼠标、键盘套装","台",11]
[null,null,"XBOX ONE Kinect 2.0","具备1080p高清摄像头、红外深度传感器和语音识别功能的体感设备，XBOX ONE Kinect 2.0","台",4]
[null,null,"Leap Motion Controller 2+XR套件","高精度手部追踪的设备，具备超低延迟、广视场角（左右 160°，上下 160°），Leap Motion Controller 2+XR套件","台",6]
[null,null,"Azure Kinect DK","1MP 深度摄像头、360˚ 麦克风阵列、12MP RGB 摄像头和方向传感器，Azure Kinect DK","台",2]
[null,null,"爱普生EH-LS650B 3LCD 4K激光投影仪","爱普生EH-LS650B 3LCD 4K激光投影仪","台",1]
[null,null,"教学电脑管理系统","具备同传，还原等功能，教学电脑管理系统","套",11]
[null,null,"学生机配套桌椅","桌子：80cm*60cm  椅子：无靠背","套",11]
[null,null,"装修设计总包","包括空间布局规划、电力与网络布设、地面、吊顶与墙面处理、光环境设计、通风温控系统、安全保障设施及部分定制化家具与环保节能设计，确保实验室功能完善、安全高效、环境舒适。","套",1]
[null,"数字动画实训室（H409）    技术咨询：马亚明13966667370","学生计算机","CPU: I Intel Core i7-13700F; GPU: NVIDIA RTX 4070 Super; 主板: ASUS TUF GAMING B660M; 内存: 32GB DDR4; 存储: 512GB NVMe SSD + 1TB HDD; 电源: 750W 或800 Gold; 散热: Thermalright(利民)；显示器：2k 24寸；鼠标、键盘套装(含同传保护)","台",41]
[null,null,"主控节点云服务器","主板：2U单路 16DM8盘位                                                             \nCPU：1颗Intel Xeon Silver 4210R\n内存：64GB DDR4\n硬盘：8T SATA +1.92TB SATA  SSD\n网卡：2*1000M\n电源：冗余电源","台",1]
[null,null,"桌面云软件-融合版","V5.0/V1.0","点",41]
[null,null,"多媒体教学软件","V9.0","套",1]
[null,null,"华腾机柜"," TC6632","台",1]
[null,null,"学生桌椅","定制","套",41]
[null,null,"电源线及综合布线","定制","项",1]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}